Release 7.1i - par H.38
Copyright (c) 1995-2005 Xilinx, Inc.  All rights reserved.

Tue May 10 17:50:34 2005


INPUT FILE:       system_map.ncd
OUTPUT FILE:      system_pad.txt
PART TYPE:        xc4vlx25
SPEED GRADE:      -10
PACKAGE:          ff668

Pinout by Pin Number:

+----------+-------------------+---------+--------------------+---------+-----------+--------------+----------+---------+-----------+---------+---------+----------+---------+-----------+----------------+
|Pin Number|Signal Name        |Pin Usage|Pin Name            |Direction|IO Standard|IO Bank Number|Drive (mA)|Slew Rate|Termination|IOB Delay|Voltage  |Constraint|DCI Value|IO Register|Signal Integrity|
+----------+-------------------+---------+--------------------+---------+-----------+--------------+----------+---------+-----------+---------+---------+----------+---------+-----------+----------------+
|A2        |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|A3        |                   |IOBM     |IO_L14P_6           |UNUSED   |           |6             |          |         |           |         |         |          |         |           |                |
|A4        |                   |IOBM     |IO_L15P_6           |UNUSED   |           |6             |          |         |           |         |         |          |         |           |                |
|A5        |gpio<6>            |IOB      |IO_L6N_6            |BIDIR    |LVCMOS25   |6             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|A6        |gpio<11>           |IOB      |IO_L6P_6            |BIDIR    |LVCMOS25   |6             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|A7        |usb_hpi_reset_n    |IOB      |IO_L3N_6            |OUTPUT   |LVCMOS25   |6             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|A8        |tft_lcd_vsync      |IOB      |IO_L3P_6            |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|A9        |phy_dv             |IOB      |IO_L13P_6           |INPUT    |LVCMOS25   |6             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|A10       |ddr_clk            |IOB      |IO_L6P_GC_LC_3      |OUTPUT   |SSTL2_I    |3             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|A11       |gpio<2>            |IOB      |IO_L2N_GC_VRP_LC_3  |BIDIR    |LVCMOS25   |3             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|A12       |gpio<3>            |IOB      |IO_L2P_GC_VRN_LC_3  |BIDIR    |LVCMOS25   |3             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|A13       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|A14       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|A15       |                   |LOWCAPIOB|IO_L5N_GC_LC_3      |UNUSED   |           |3             |          |         |           |         |         |          |         |           |                |
|A16       |ddr_ba<1>          |IOB      |IO_L5P_GC_LC_3      |OUTPUT   |SSTL2_I    |3             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|A17       |iic_scl            |IOB      |IO_L7N_GC_LC_3      |BIDIR    |LVCMOS25   |3             |6         |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|A18       |ddr_ad<10>         |IOB      |IO_L3N_5            |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|A19       |ddr_dq<17>         |IOB      |IO_L13N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|A20       |ddr_dq<12>         |IOB      |IO_L13P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|A21       |ddr_dq<13>         |IOB      |IO_L15N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|A22       |ddr_dq<9>          |IOB      |IO_L15P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|A23       |ddr_web            |IOB      |IO_L8N_CC_LC_5      |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|A24       |ddr_ad<12>         |IOB      |IO_L8P_CC_LC_5      |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|A25       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AA1       |sram_flash_addr<2> |IOB      |IO_L10N_8           |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AA2       |                   |         |VCCO_8              |         |           |8             |          |         |           |         |3.30     |          |         |           |                |
|AA3       |sram_flash_addr<14>|IOB      |IO_L7N_8            |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AA4       |sram_flash_addr<15>|IOB      |IO_L7P_8            |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AA5       |                   |         |VCCO_8              |         |           |8             |          |         |           |         |3.30     |          |         |           |                |
|AA6       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AA7       |sace_usb_d<15>     |IOB      |IO_L20P_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AA8       |sace_usb_oen       |IOB      |IO_L26P_8           |OUTPUT   |LVCMOS33   |8             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|AA9       |sace_usb_a<5>      |IOB      |IO_L21P_8           |OUTPUT   |LVCMOS33   |8             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|AA10      |sace_usb_a<2>      |IOB      |IO_L27N_8           |OUTPUT   |LVCMOS33   |8             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|AA11      |sram_flash_data<4> |IOB      |IO_L6N_D4_LC_2      |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AA12      |sram_flash_data<5> |IOB      |IO_L6P_D5_LC_2      |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AA13      |sram_flash_data<8> |IOB      |IO_L4N_D8_VREF_LC_2 |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AA14      |sram_flash_data<15>|IOB      |IO_L1P_D15_CC_LC_2  |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AA15      |sram_flash_data<10>|IOB      |IO_L3N_D10_LC_2     |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AA16      |sram_flash_data<11>|IOB      |IO_L3P_D11_LC_2     |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AA17      |gpio_exp_hdr2<12>  |IOB      |IO_L27N_SM5_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AA18      |gpio_exp_hdr2<1>   |IOB      |IO_L21P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AA19      |gpio_exp_hdr2<11>  |IOB      |IO_L26P_SM6_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AA20      |gpio_exp_hdr2<10>  |IOB      |IO_L26N_SM6_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AA21      |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AA22      |                   |         |VCCO_7              |         |           |7             |          |         |           |         |2.50     |          |         |           |                |
|AA23      |gpio_exp_hdr1<12>  |IOB      |IO_L14N_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AA24      |gpio_exp_hdr1<0>   |IOB      |IO_L8P_CC_LC_7      |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AA25      |                   |         |VCCO_7              |         |           |7             |          |         |           |         |2.50     |          |         |           |                |
|AA26      |gpio_exp_hdr1<11>  |IOB      |IO_L10N_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB1       |sram_flash_addr<3> |IOB      |IO_L10P_8           |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AB2       |sram_flash_addr<4> |IOB      |IO_L12N_VREF_8      |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AB3       |sram_flash_addr<16>|IOB      |IO_L12P_8           |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AB4       |sram_flash_addr<17>|IOB      |IO_L11N_8           |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AB5       |sram_flash_addr<19>|IOB      |IO_L13N_8           |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AB6       |sram_flash_we_n    |IOB      |IO_L24N_CC_LC_8     |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AB7       |sace_usb_d<0>      |IOB      |IO_L28N_VREF_8      |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB8       |                   |         |VCCO_8              |         |           |8             |          |         |           |         |3.30     |          |         |           |                |
|AB9       |sace_usb_d<2>      |IOB      |IO_L29N_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB10      |gpio_char_lcd<0>   |IOB      |IO_L2N_GC_LC_4      |BIDIR    |LVCMOS33   |4             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB11      |                   |         |VCCO_2              |         |           |2             |          |         |           |         |3.30     |          |         |           |                |
|AB12      |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AB13      |sram_flash_data<9> |IOB      |IO_L4P_D9_LC_2      |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB14      |sram_flash_data<14>|IOB      |IO_L1N_D14_CC_LC_2  |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB15      |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AB16      |                   |         |VCCO_2              |         |           |2             |          |         |           |         |3.30     |          |         |           |                |
|AB17      |gpio_char_lcd<4>   |IOB      |IO_L3P_GC_LC_4      |BIDIR    |LVCMOS33   |4             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB18      |gpio_exp_hdr2<22>  |IOB      |IO_L29N_SM4_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB19      |                   |         |VCCO_7              |         |           |7             |          |         |           |         |2.50     |          |         |           |                |
|AB20      |gpio_exp_hdr2<15>  |IOB      |IO_L28P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB21      |gpio_exp_hdr1<28>  |IOB      |IO_L24N_CC_LC_7     |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB22      |gpio_exp_hdr1<25>  |IOB      |IO_L13N_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB23      |gpio_exp_hdr1<7>   |IOB      |IO_L14P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB24      |gpio_exp_hdr1<5>   |IOB      |IO_L7P_7            |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB25      |gpio_exp_hdr1<16>  |IOB      |IO_L7N_7            |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AB26      |gpio_exp_hdr1<14>  |IOB      |IO_L10P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC1       |sram_flash_addr<5> |IOB      |IO_L14N_8           |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AC2       |sram_flash_addr<6> |IOB      |IO_L14P_8           |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AC3       |sace_usb_d<12>     |IOB      |IO_L18N_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC4       |sram_flash_addr<18>|IOB      |IO_L11P_8           |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AC5       |sram_flash_addr<20>|IOB      |IO_L13P_8           |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AC6       |sram_flash_oe_n    |IOB      |IO_L24P_CC_LC_8     |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AC7       |sace_usb_a<3>      |IOB      |IO_L28P_8           |OUTPUT   |LVCMOS33   |8             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|AC8       |sace_usb_d<8>      |IOB      |IO_L32N_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC9       |sace_usb_d<1>      |IOB      |IO_L29P_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC10      |gpio_char_lcd<1>   |IOB      |IO_L2P_GC_LC_4      |BIDIR    |LVCMOS33   |4             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC11      |sram_flash_data<12>|IOB      |IO_L2N_D12_LC_2     |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC12      |sram_flash_data<13>|IOB      |IO_L2P_D13_LC_2     |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC13      |sram_flash_data<1> |IOB      |IO_L8P_D1_LC_2      |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC14      |sram_flash_data<7> |IOB      |IO_L5P_D7_LC_2      |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC15      |sram_flash_data<2> |IOB      |IO_L7N_D2_LC_2      |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC16      |sram_flash_data<3> |IOB      |IO_L7P_D3_LC_2      |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC17      |gpio_char_lcd<5>   |IOB      |IO_L3N_GC_LC_4      |BIDIR    |LVCMOS33   |4             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC18      |gpio_exp_hdr2<23>  |IOB      |IO_L29P_SM4_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC19      |gpio_exp_hdr2<20>  |IOB      |IO_L25N_CC_SM7_LC_7 |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC20      |gpio_exp_hdr2<14>  |IOB      |IO_L28N_VREF_7      |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC21      |gpio_exp_hdr1<13>  |IOB      |IO_L24P_CC_LC_7     |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC22      |gpio_exp_hdr1<20>  |IOB      |IO_L13P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC23      |gpio_exp_hdr1<15>  |IOB      |IO_L16P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC24      |gpio_exp_hdr1<3>   |IOB      |IO_L16N_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC25      |gpio_exp_hdr1<2>   |IOB      |IO_L9P_CC_LC_7      |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AC26      |gpio_exp_hdr1<18>  |IOB      |IO_L9N_CC_LC_7      |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD1       |sram_flash_addr<7> |IOB      |IO_L16N_8           |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AD2       |sram_flash_addr<8> |IOB      |IO_L16P_8           |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AD3       |sace_usb_d<11>     |IOB      |IO_L18P_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD4       |sysace_mpirq       |IOB      |IO_L22N_8           |INPUT    |LVCMOS33   |8             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD5       |sace_mpce          |IOB      |IO_L22P_8           |OUTPUT   |LVCMOS33   |8             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|AD6       |sace_usb_d<4>      |IOB      |IO_L30N_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD7       |                   |IOBS     |IO_L23N_VRP_8       |UNUSED   |           |8             |          |         |           |         |         |          |         |           |                |
|AD8       |sace_usb_d<7>      |IOB      |IO_L32P_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD9       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AD10      |ac97_reset_n       |IOB      |IO_L6N_GC_LC_4      |OUTPUT   |LVCMOS33   |4             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|AD11      |                   |LOWCAPIOB|IO_L8N_GC_CC_LC_4   |UNUSED   |           |4             |          |         |           |         |         |          |         |           |                |
|AD12      |gpio<26>           |IOB      |IO_L8P_GC_CC_LC_4   |BIDIR    |LVCMOS33   |4             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD13      |sram_flash_data<0> |IOB      |IO_L8N_D0_LC_2      |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD14      |sram_flash_data<6> |IOB      |IO_L5N_D6_LC_2      |BIDIR    |LVCMOS33   |2             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD15      |                   |         |VCCO_4              |         |           |4             |          |         |           |         |3.30     |          |         |           |                |
|AD16      |ac97_sdata_In      |IOB      |IO_L7N_GC_VRP_LC_4  |INPUT    |LVCMOS33   |4             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD17      |sram_clk_fb        |IOB      |IO_L7P_GC_VRN_LC_4  |INPUT    |LVCMOS33   |4             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD18      |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AD19      |gpio_exp_hdr2<21>  |IOB      |IO_L25P_CC_SM7_LC_7 |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD20      |gpio_exp_hdr2<18>  |IOB      |IO_L23N_VRP_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD21      |gpio_exp_hdr2<16>  |IOB      |IO_L32N_SM1_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD22      |gpio_exp_hdr1<29>  |IOB      |IO_L15P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD23      |gpio_exp_hdr1<17>  |IOB      |IO_L15N_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD24      |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AD25      |gpio_exp_hdr1<24>  |IOB      |IO_L11P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AD26      |gpio_exp_hdr1<19>  |IOB      |IO_L11N_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AE1       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AE2       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AE3       |sram_flash_addr<9> |IOB      |IO_L15N_8           |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AE4       |sace_usb_d<10>     |IOB      |IO_L17N_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AE5       |                   |         |VCCO_8              |         |           |8             |          |         |           |         |3.30     |          |         |           |                |
|AE6       |sace_usb_d<3>      |IOB      |IO_L30P_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AE7       |                   |IOBM     |IO_L23P_VRN_8       |UNUSED   |           |8             |          |         |           |         |         |          |         |           |                |
|AE8       |                   |         |VCCO_8              |         |           |8             |          |         |           |         |3.30     |          |         |           |                |
|AE9       |sace_usb_d<6>      |IOB      |IO_L31N_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AE10      |ac97_bit_clk       |IOB      |IO_L6P_GC_LC_4      |INPUT    |LVCMOS33   |4             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|AE11      |                   |         |VCCO_4              |         |           |4             |          |         |           |         |3.30     |          |         |           |                |
|AE12      |gpio_char_lcd<2>   |IOB      |IO_L1N_GC_LC_4      |BIDIR    |LVCMOS33   |4             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AE13      |gpio_char_lcd<6>   |IOB      |IO_L5N_GC_LC_4      |BIDIR    |LVCMOS33   |4             |12        |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|AE14      |sys_clk_in         |IOB      |IO_L5P_GC_LC_4      |INPUT    |LVCMOS33   |4             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|AE15      |                   |         |VREFN_SM            |         |           |              |          |         |           |         |         |          |         |           |                |
|AE16      |                   |         |VREFP_SM            |         |           |              |          |         |           |         |         |          |         |           |                |
|AE17      |                   |         |AVSS_SM             |         |           |              |          |         |           |         |         |          |         |           |                |
|AE18      |gpio_exp_hdr2<30>  |IOB      |IO_L31N_SM2_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AE19      |                   |         |VCCO_7              |         |           |7             |          |         |           |         |2.50     |          |         |           |                |
|AE20      |gpio_exp_hdr2<19>  |IOB      |IO_L23P_VRN_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AE21      |gpio_exp_hdr2<17>  |IOB      |IO_L32P_SM1_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AE22      |                   |         |VCCO_7              |         |           |7             |          |         |           |         |2.50     |          |         |           |                |
|AE23      |gpio_exp_hdr2<24>  |IOB      |IO_L19N_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AE24      |gpio_exp_hdr1<30>  |IOB      |IO_L22N_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AE25      |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AE26      |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AF2       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AF3       |sram_flash_addr<10>|IOB      |IO_L15P_8           |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AF4       |sace_usb_d<9>      |IOB      |IO_L17P_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AF5       |sace_usb_d<14>     |IOB      |IO_L19N_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AF6       |sace_usb_d<13>     |IOB      |IO_L19P_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AF7       |sram_clk           |IOB      |IO_L25N_CC_LC_8     |OUTPUT   |LVCMOS33   |8             |16        |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|AF8       |tft_lcd_clk        |IOB      |IO_L25P_CC_LC_8     |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|AF9       |sace_usb_d<5>      |IOB      |IO_L31P_8           |BIDIR    |LVCMOS33   |8             |8         |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AF10      |usb_csn            |IOB      |IO_L4N_GC_VREF_LC_4 |OUTPUT   |LVCMOS33   |4             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|AF11      |sysace_clk_in      |IOB      |IO_L4P_GC_LC_4      |INPUT    |LVCMOS33   |4             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|AF12      |gpio_char_lcd<3>   |IOB      |IO_L1P_GC_LC_4      |BIDIR    |LVCMOS33   |4             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AF13      |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AF14      |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|AF15      |                   |IPAD     |VN_SM               |UNUSED   |           |              |          |         |           |         |         |          |         |           |                |
|AF16      |                   |IPAD     |VP_SM               |UNUSED   |           |              |          |         |           |         |         |          |         |           |                |
|AF17      |                   |         |AVDD_SM             |         |           |              |          |         |           |         |         |          |         |           |                |
|AF18      |gpio_exp_hdr2<31>  |IOB      |IO_L31P_SM2_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AF19      |gpio_exp_hdr2<29>  |IOB      |IO_L17P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AF20      |gpio_exp_hdr2<28>  |IOB      |IO_L17N_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AF21      |gpio_exp_hdr2<27>  |IOB      |IO_L30P_SM3_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AF22      |gpio_exp_hdr2<26>  |IOB      |IO_L30N_SM3_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AF23      |gpio_exp_hdr2<25>  |IOB      |IO_L19P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AF24      |gpio_exp_hdr1<31>  |IOB      |IO_L22P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|AF25      |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|B1        |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|B2        |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|B3        |                   |IOBS     |IO_L14N_6           |UNUSED   |           |6             |          |         |           |         |         |          |         |           |                |
|B4        |                   |IOBS     |IO_L15N_6           |UNUSED   |           |6             |          |         |           |         |         |          |         |           |                |
|B5        |                   |         |VCCO_6              |         |           |6             |          |         |           |         |2.50     |          |         |           |                |
|B6        |gpio<9>            |IOB      |IO_L8P_CC_LC_6      |BIDIR    |LVCMOS25   |6             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|B7        |tft_lcd_b<3>       |IOB      |IO_L11P_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|B8        |                   |         |VCCO_6              |         |           |6             |          |         |           |         |2.50     |          |         |           |                |
|B9        |phy_rx_er          |IOB      |IO_L13N_6           |INPUT    |LVCMOS25   |6             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|B10       |ddr_clkb           |IOB      |IO_L6N_GC_LC_3      |OUTPUT   |SSTL2_I    |3             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|B11       |                   |         |VCCO_3              |         |           |3             |          |         |           |         |2.50     |          |         |           |                |
|B12       |ddr_ba<0>          |IOB      |IO_L4N_GC_VREF_LC_3 |OUTPUT   |SSTL2_I    |3             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|B13       |ddr_clk_fb         |IOB      |IO_L4P_GC_LC_3      |INPUT    |LVCMOS25   |3             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|B14       |ps2_mouse_clk      |IOB      |IO_L1N_GC_CC_LC_3   |BIDIR    |LVCMOS25   |3             |2         |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|B15       |phy_rx_clk         |IOB      |IO_L1P_GC_CC_LC_3   |INPUT    |LVCMOS25   |3             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|B16       |                   |         |VCCO_3              |         |           |3             |          |         |           |         |2.50     |          |         |           |                |
|B17       |iic_sda            |IOB      |IO_L7P_GC_LC_3      |BIDIR    |LVCMOS25   |3             |6         |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|B18       |ddr_ad<5>          |IOB      |IO_L3P_5            |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|B19       |                   |         |VCCO_5              |         |           |5             |          |         |           |         |2.50     |          |         |           |                |
|B20       |ddr_ad<6>          |IOB      |IO_L2N_5            |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|B21       |ddr_ad<11>         |IOB      |IO_L6N_5            |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|B22       |                   |         |VCCO_5              |         |           |5             |          |         |           |         |2.50     |          |         |           |                |
|B23       |ddr_dq<19>         |IOB      |IO_L10N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|B24       |ddr_dq<23>         |IOB      |IO_L10P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|B25       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|B26       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|C1        |tft_lcd_g<5>       |IOB      |IO_L20N_VREF_6      |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|C2        |tft_lcd_r<1>       |IOB      |IO_L20P_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|C3        |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|C4        |phy_rx_data<3>     |IOB      |IO_L16P_6           |INPUT    |LVCMOS25   |6             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|C5        |tft_lcd_b<1>       |IOB      |IO_L12P_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|C6        |gpio<4>            |IOB      |IO_L8N_CC_LC_6      |BIDIR    |LVCMOS25   |6             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|C7        |tft_lcd_b<2>       |IOB      |IO_L11N_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|C8        |ac97_sdata_Out     |IOB      |IO_L2N_6            |OUTPUT   |LVCMOS25   |6             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|C9        |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|C10       |tft_lcd_hsync      |IOB      |IO_L1N_6            |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|C11       |sram_flash_data<21>|IOB      |IO_L6P_D21_LC_1     |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|C12       |gpio<22>           |IOB      |IO_L8N_GC_LC_3      |BIDIR    |LVCMOS25   |3             |12        |FAST     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|C13       |gpio<23>           |IOB      |IO_L8P_GC_LC_3      |BIDIR    |LVCMOS25   |3             |12        |FAST     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|C14       |ps2_mouse_data     |IOB      |IO_L3N_GC_LC_3      |BIDIR    |LVCMOS25   |3             |2         |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|C15       |phy_tx_clk         |IOB      |IO_L3P_GC_LC_3      |INPUT    |LVCMOS25   |3             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|C16       |sram_flash_data<18>|IOB      |IO_L7N_D18_LC_1     |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|C17       |                   |IOBM     |IO_L1P_5            |UNUSED   |           |5             |          |         |           |         |         |          |         |           |                |
|C18       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|C19       |ddr_ad<3>          |IOB      |IO_L7P_5            |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|C20       |ddr_ad<7>          |IOB      |IO_L2P_5            |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|C21       |ddr_ad<9>          |IOB      |IO_L6P_5            |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|C22       |ddr_dm<3>          |IOB      |IO_L14N_5           |OUTPUT   |SSTL2_II   |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|C23       |ddr_dq<10>         |IOB      |IO_L21N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|C24       |ddr_dq<11>         |IOB      |IO_L16N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|C25       |                   |IOBS     |IO_L20N_VREF_5      |UNUSED   |           |5             |          |         |           |         |1.25     |          |         |           |                |
|C26       |ddr_ad<0>          |IOB      |IO_L20P_5           |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|D1        |phy_mii_clk        |IOB      |IO_L25N_CC_LC_6     |TRISTATE |LVCMOS25   |6             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|D2        |ps2_keyb_clk       |IOB      |IO_L25P_CC_LC_6     |BIDIR    |LVCMOS25   |6             |2         |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|D3        |tft_lcd_g<2>       |IOB      |IO_L22P_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|D4        |phy_rx_data<2>     |IOB      |IO_L16N_6           |INPUT    |LVCMOS25   |6             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|D5        |phy_crs            |IOB      |IO_L12N_VREF_6      |INPUT    |LVCMOS25   |6             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|D6        |sys_rst_in         |IOB      |IO_L17N_6           |INPUT    |LVCMOS25   |6             |          |         |PULLUP     |NONE     |         |LOCATED   |         |NO         |NONE            |
|D7        |gpio<24>           |IOB      |IO_L4N_VREF_6       |BIDIR    |LVCMOS25   |6             |12        |FAST     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|D8        |gpio<25>           |IOB      |IO_L4P_6            |BIDIR    |LVCMOS25   |6             |12        |FAST     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|D9        |ac97_sync          |IOB      |IO_L2P_6            |OUTPUT   |LVCMOS25   |6             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|D10       |phy_rst_n          |IOB      |IO_L1P_6            |OUTPUT   |LVCMOS25   |6             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|D11       |sram_flash_data<20>|IOB      |IO_L6N_D20_LC_1     |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|D12       |sram_flash_data<16>|IOB      |IO_L8N_D16_CC_LC_1  |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|D13       |sram_flash_data<24>|IOB      |IO_L4N_D24_VREF_LC_1|BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|D14       |sram_flash_data<25>|IOB      |IO_L4P_D25_LC_1     |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|D15       |sram_flash_data<23>|IOB      |IO_L5P_D23_LC_1     |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|D16       |sram_flash_data<19>|IOB      |IO_L7P_D19_LC_1     |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|D17       |                   |IOBS     |IO_L1N_5            |UNUSED   |           |5             |          |         |           |         |         |          |         |           |                |
|D18       |ddr_ad<2>          |IOB      |IO_L7N_5            |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|D19       |                   |IOBS     |IO_L4N_VREF_5       |UNUSED   |           |5             |          |         |           |         |1.25     |          |         |           |                |
|D20       |ddr_ad<8>          |IOB      |IO_L4P_5            |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|D21       |                   |IOBS     |IO_L12N_VREF_5      |UNUSED   |           |5             |          |         |           |         |1.25     |          |         |           |                |
|D22       |ddr_dq<21>         |IOB      |IO_L14P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|D23       |ddr_dq<22>         |IOB      |IO_L21P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|D24       |ddr_dq<14>         |IOB      |IO_L16P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|D25       |ddr_dqs<0>         |IOB      |IO_L25N_CC_LC_5     |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|D26       |ddr_dqs<3>         |IOB      |IO_L25P_CC_LC_5     |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|E1        |phy_rx_data<1>     |IOB      |IO_L26P_6           |INPUT    |LVCMOS25   |6             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|E2        |gpio<8>            |IOB      |IO_L24N_CC_LC_6     |BIDIR    |LVCMOS25   |6             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|E3        |phy_col            |IOB      |IO_L24P_CC_LC_6     |INPUT    |LVCMOS25   |6             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|E4        |tft_lcd_g<1>       |IOB      |IO_L22N_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|E5        |tft_lcd_r<4>       |IOB      |IO_L18N_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|E6        |tft_lcd_r<5>       |IOB      |IO_L18P_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|E7        |gpio<13>           |IOB      |IO_L17P_6           |BIDIR    |LVCMOS25   |6             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|E8        |                   |         |VCCO_6              |         |           |6             |          |         |           |         |2.50     |          |         |           |                |
|E9        |gpio<10>           |IOB      |IO_L7P_6            |BIDIR    |LVCMOS25   |6             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|E10       |gpio<7>            |IOB      |IO_L5N_6            |BIDIR    |LVCMOS25   |6             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|E11       |                   |         |VCCO_1              |         |           |1             |          |         |           |         |3.30     |          |         |           |                |
|E12       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|E13       |sram_flash_data<17>|IOB      |IO_L8P_D17_CC_LC_1  |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|E14       |sram_flash_data<22>|IOB      |IO_L5N_D22_LC_1     |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|E15       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|E16       |                   |         |VCCO_1              |         |           |1             |          |         |           |         |3.30     |          |         |           |                |
|E17       |ddr_ad<1>          |IOB      |IO_L5P_5            |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|E18       |ddr_dq<15>         |IOB      |IO_L11N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|E19       |                   |         |VCCO_5              |         |           |5             |          |         |           |         |2.50     |          |         |           |                |
|E20       |ddr_dq<8>          |IOB      |IO_L19N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|E21       |ddr_dq<20>         |IOB      |IO_L12P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|E22       |ddr_dq<24>         |IOB      |IO_L18N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|E23       |ddr_dq<1>          |IOB      |IO_L18P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|E24       |ddr_dq<7>          |IOB      |IO_L27N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|E25       |ddr_dq<4>          |IOB      |IO_L27P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|E26       |ddr_dq<5>          |IOB      |IO_L29N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|F1        |phy_rx_data<0>     |IOB      |IO_L26N_6           |INPUT    |LVCMOS25   |6             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|F2        |                   |         |VCCO_6              |         |           |6             |          |         |           |         |2.50     |          |         |           |                |
|F3        |phy_tx_er          |IOB      |IO_L27N_6           |OUTPUT   |LVCMOS25   |6             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|F4        |phy_tx_en          |IOB      |IO_L27P_6           |OUTPUT   |LVCMOS25   |6             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|F5        |                   |         |VCCO_6              |         |           |6             |          |         |           |         |2.50     |          |         |           |                |
|F6        |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|F7        |tft_lcd_r<3>       |IOB      |IO_L19P_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|F8        |tft_lcd_b<5>       |IOB      |IO_L10P_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|F9        |gpio<5>            |IOB      |IO_L7N_6            |BIDIR    |LVCMOS25   |6             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|F10       |gpio<12>           |IOB      |IO_L5P_6            |BIDIR    |LVCMOS25   |6             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|F11       |sram_flash_data<28>|IOB      |IO_L2N_D28_LC_1     |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|F12       |sram_flash_data<29>|IOB      |IO_L2P_D29_LC_1     |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|F13       |sram_flash_data<30>|IOB      |IO_L1N_D30_LC_1     |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|F14       |sram_flash_data<31>|IOB      |IO_L1P_D31_LC_1     |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|F15       |sram_flash_data<26>|IOB      |IO_L3N_D26_LC_1     |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|F16       |sram_flash_data<27>|IOB      |IO_L3P_D27_LC_1     |BIDIR    |LVCMOS33   |1             |12        |FAST     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|F17       |ddr_ad<4>          |IOB      |IO_L5N_5            |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|F18       |ddr_dq<16>         |IOB      |IO_L11P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|F19       |ddr_dq<18>         |IOB      |IO_L17N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|F20       |ddr_dq<25>         |IOB      |IO_L19P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|F21       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|F22       |                   |         |VCCO_5              |         |           |5             |          |         |           |         |2.50     |          |         |           |                |
|F23       |ddr_casb           |IOB      |IO_L24N_CC_LC_5     |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|F24       |ddr_rasb           |IOB      |IO_L24P_CC_LC_5     |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|F25       |                   |         |VCCO_5              |         |           |5             |          |         |           |         |2.50     |          |         |           |                |
|F26       |ddr_dq<6>          |IOB      |IO_L29P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|G1        |phy_tx_data<3>     |IOB      |IO_L30N_6           |OUTPUT   |LVCMOS25   |6             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|G2        |                   |IOBM     |IO_L30P_6           |UNUSED   |           |6             |          |         |           |         |         |          |         |           |                |
|G3        |                   |IOBS     |IO_L28N_VREF_6      |UNUSED   |           |6             |          |         |           |         |         |          |         |           |                |
|G4        |phy_mii_data       |IOB      |IO_L28P_6           |BIDIR    |LVCMOS25   |6             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|G5        |gpio<0>            |IOB      |IO_L23N_VRP_6       |BIDIR    |LVCMOS25   |6             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|G6        |gpio<1>            |IOB      |IO_L23P_VRN_6       |BIDIR    |LVCMOS25   |6             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|G7        |tft_lcd_r<2>       |IOB      |IO_L19N_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|G8        |tft_lcd_b<4>       |IOB      |IO_L10N_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|G9        |ps2_keyb_data      |IOB      |IO_L9N_CC_LC_6      |BIDIR    |LVCMOS25   |6             |2         |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|G10       |                   |LOWCAPIOB|IO_L9P_CC_LC_6      |UNUSED   |           |6             |          |         |           |         |         |          |         |           |                |
|G11       |                   |         |CS_B_0              |         |           |              |          |         |           |         |         |          |         |           |                |
|G12       |                   |         |D_IN_0              |         |           |              |          |         |           |         |         |          |         |           |                |
|G13       |                   |         |TDN_0               |         |           |              |          |         |           |         |         |          |         |           |                |
|G14       |                   |         |CCLK_0              |         |           |              |          |         |           |         |         |          |         |           |                |
|G15       |                   |         |INIT_0              |         |           |              |          |         |           |         |         |          |         |           |                |
|G16       |                   |         |HSWAPEN_0           |         |           |              |          |         |           |         |         |          |         |           |                |
|G17       |ddr_dqs<2>         |IOB      |IO_L9N_CC_LC_5      |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|G18       |ddr_dqs<1>         |IOB      |IO_L9P_CC_LC_5      |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|G19       |ddr_dm<0>          |IOB      |IO_L17P_5           |OUTPUT   |SSTL2_II   |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|G20       |ddr_dm<2>          |IOB      |IO_L22N_5           |OUTPUT   |SSTL2_II   |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|G21       |ddr_csb            |IOB      |IO_L23N_VRP_5       |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|G22       |ddr_cke            |IOB      |IO_L23P_VRN_5       |OUTPUT   |SSTL2_I    |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|G23       |                   |IOBS     |IO_L28N_VREF_5      |UNUSED   |           |5             |          |         |           |         |1.25     |          |         |           |                |
|G24       |ddr_dm<1>          |IOB      |IO_L28P_5           |OUTPUT   |SSTL2_II   |5             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|G25       |ddr_dq<27>         |IOB      |IO_L31N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|G26       |ddr_dq<28>         |IOB      |IO_L31P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|H1        |phy_tx_data<0>     |IOB      |IO_L32N_6           |OUTPUT   |LVCMOS25   |6             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|H2        |phy_tx_data<1>     |IOB      |IO_L32P_6           |OUTPUT   |LVCMOS25   |6             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|H3        |phy_tx_data<2>     |IOB      |IO_L31N_6           |OUTPUT   |LVCMOS25   |6             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|H4        |phy_mii_int_n      |IOB      |IO_L31P_6           |INPUT    |LVCMOS25   |6             |          |         |PULLUP     |NONE     |         |LOCATED   |         |NO         |NONE            |
|H5        |                   |IOBS     |IO_L29N_6           |UNUSED   |           |6             |          |         |           |         |         |          |         |           |                |
|H6        |                   |IOBM     |IO_L29P_6           |UNUSED   |           |6             |          |         |           |         |         |          |         |           |                |
|H7        |tft_lcd_g<3>       |IOB      |IO_L21N_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|H8        |tft_lcd_g<4>       |IOB      |IO_L21P_6           |OUTPUT   |LVCMOS25   |6             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|H9        |                   |         |VCCO_6              |         |           |6             |          |         |           |         |2.50     |          |         |           |                |
|H10       |                   |         |VCCO_6              |         |           |6             |          |         |           |         |2.50     |          |         |           |                |
|H11       |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|H12       |                   |         |RDWR_B_0            |         |           |              |          |         |           |         |         |          |         |           |                |
|H13       |                   |         |TDP_0               |         |           |              |          |         |           |         |         |          |         |           |                |
|H14       |                   |         |DONE_0              |         |           |              |          |         |           |         |         |          |         |           |                |
|H15       |                   |         |PROGRAM_B_0         |         |           |              |          |         |           |         |         |          |         |           |                |
|H16       |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|H17       |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|H18       |                   |         |VCCO_5              |         |           |5             |          |         |           |         |2.50     |          |         |           |                |
|H19       |                   |         |VCCO_5              |         |           |5             |          |         |           |         |2.50     |          |         |           |                |
|H20       |ddr_dq<0>          |IOB      |IO_L22P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|H21       |ddr_dq<31>         |IOB      |IO_L26N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|H22       |ddr_dq<3>          |IOB      |IO_L26P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|H23       |ddr_dq<26>         |IOB      |IO_L30N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|H24       |ddr_dq<30>         |IOB      |IO_L30P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|H25       |ddr_dq<29>         |IOB      |IO_L32N_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|H26       |ddr_dq<2>          |IOB      |IO_L32P_5           |BIDIR    |SSTL2_II   |5             |          |NONE*    |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|J1        |                   |IOBS     |IO_L4N_VREF_10      |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|J2        |                   |IOBM     |IO_L4P_10           |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|J3        |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|J4        |                   |IOBS     |IO_L2N_10           |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|J5        |                   |IOBM     |IO_L2P_10           |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|J6        |                   |IOBS     |IO_L1N_10           |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|J7        |                   |IOBM     |IO_L1P_10           |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|J8        |                   |         |VCCO_6              |         |           |6             |          |         |           |         |2.50     |          |         |           |                |
|J10       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|J11       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|J12       |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|J13       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|J14       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|J15       |                   |         |VCCO_0              |         |           |0             |          |         |           |         |any******|          |         |           |                |
|J16       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|J17       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|J19       |                   |         |VCCO_5              |         |           |5             |          |         |           |         |2.50     |          |         |           |                |
|J20       |                   |IOBS     |IO_L1N_9            |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|J21       |                   |IOBM     |IO_L1P_9            |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|J22       |                   |IOBS     |IO_L2N_9            |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|J23       |                   |IOBM     |IO_L2P_9            |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|J24       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|J25       |                   |IOBS     |IO_L4N_VREF_9       |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|J26       |                   |IOBM     |IO_L4P_9            |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|K1        |                   |IOBS     |IO_L10N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|K2        |                   |IOBS     |IO_L7N_10           |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|K3        |                   |IOBM     |IO_L7P_10           |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|K4        |                   |IOBS     |IO_L6N_10           |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|K5        |                   |IOBM     |IO_L6P_10           |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|K6        |                   |IOBS     |IO_L3N_10           |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|K7        |                   |IOBM     |IO_L3P_10           |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|K8        |                   |         |VCCO_10             |         |           |10            |          |         |           |         |any******|          |         |           |                |
|K9        |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|K10       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|K11       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|K12       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|K13       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|K14       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|K15       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|K16       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|K17       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|K18       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|K19       |                   |         |VCCO_9              |         |           |9             |          |         |           |         |3.30     |          |         |           |                |
|K20       |                   |IOBS     |IO_L5N_9            |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|K21       |                   |IOBS     |IO_L3N_9            |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|K22       |                   |IOBM     |IO_L3P_9            |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|K23       |                   |IOBS     |IO_L7N_9            |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|K24       |                   |IOBM     |IO_L7P_9            |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|K25       |                   |LOWCAPIOB|IO_L8N_CC_LC_9      |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|K26       |                   |LOWCAPIOB|IO_L8P_CC_LC_9      |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|L1        |                   |IOBM     |IO_L10P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|L2        |                   |         |VCCO_10             |         |           |10            |          |         |           |         |any******|          |         |           |                |
|L3        |                   |LOWCAPIOB|IO_L8N_CC_LC_10     |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|L4        |                   |LOWCAPIOB|IO_L8P_CC_LC_10     |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|L5        |                   |         |VCCO_10             |         |           |10            |          |         |           |         |any******|          |         |           |                |
|L6        |                   |IOBS     |IO_L5N_10           |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|L7        |                   |IOBM     |IO_L5P_10           |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|L8        |                   |LOWCAPIOB|IO_L9N_CC_LC_10     |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|L9        |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|L10       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|L11       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|L12       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|L13       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|L14       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|L15       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|L16       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|L17       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|L18       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|L19       |                   |IOBM     |IO_L5P_9            |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|L20       |                   |IOBS     |IO_L6N_9            |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|L21       |                   |IOBM     |IO_L6P_9            |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|L22       |                   |         |VCCO_9              |         |           |9             |          |         |           |         |3.30     |          |         |           |                |
|L23       |                   |IOBS     |IO_L10N_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|L24       |plb_error          |IOB      |IO_L10P_9           |OUTPUT   |LVCMOS33   |9             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|L25       |                   |         |VCCO_9              |         |           |9             |          |         |           |         |3.30     |          |         |           |                |
|L26       |tft_lcd_b<0>       |IOB      |IO_L12P_9           |OUTPUT   |LVCMOS33   |9             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|M1        |                   |IOBS     |IO_L11N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|M2        |                   |IOBM     |IO_L11P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|M3        |                   |IOBS     |IO_L12N_VREF_10     |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|M4        |                   |IOBM     |IO_L12P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|M5        |                   |IOBS     |IO_L13N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|M6        |                   |IOBM     |IO_L13P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|M7        |                   |IOBS     |IO_L17N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|M8        |                   |LOWCAPIOB|IO_L9P_CC_LC_10     |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|M9        |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|M10       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|M11       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|M12       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|M13       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|M14       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|M15       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|M16       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|M17       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|M18       |                   |         |VCCO_9              |         |           |9             |          |         |           |         |3.30     |          |         |           |                |
|M19       |                   |LOWCAPIOB|IO_L9P_CC_LC_9      |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|M20       |tft_lcd_g<0>       |IOB      |IO_L13N_9           |OUTPUT   |LVCMOS33   |9             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|M21       |                   |IOBM     |IO_L13P_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|M22       |                   |IOBS     |IO_L14N_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|M23       |                   |IOBM     |IO_L14P_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|M24       |                   |IOBS     |IO_L11N_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|M25       |                   |IOBM     |IO_L11P_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|M26       |                   |IOBS     |IO_L12N_VREF_9      |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|N1        |                   |         |VCCO_10             |         |           |10            |          |         |           |         |any******|          |         |           |                |
|N2        |                   |IOBS     |IO_L14N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|N3        |                   |IOBM     |IO_L14P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|N4        |                   |IOBS     |IO_L15N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|N5        |                   |IOBM     |IO_L15P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|N6        |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|N7        |                   |IOBM     |IO_L17P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|N8        |                   |IOBS     |IO_L19N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|N9        |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|N10       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|N11       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|N12       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|N13       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|N14       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|N15       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|N16       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|N17       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|N18       |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|N19       |                   |LOWCAPIOB|IO_L9N_CC_LC_9      |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|N20       |                   |IOBS     |IO_L17N_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|N21       |                   |IOBM     |IO_L17P_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|N22       |                   |IOBS     |IO_L16N_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|N23       |                   |IOBM     |IO_L16P_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|N24       |                   |IOBS     |IO_L15N_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|N25       |tft_lcd_r<0>       |IOB      |IO_L15P_9           |OUTPUT   |LVCMOS33   |9             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|N26       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|P1        |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|P2        |                   |IOBS     |IO_L16N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|P3        |                   |IOBM     |IO_L16P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|P4        |                   |IOBS     |IO_L18N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|P5        |                   |IOBM     |IO_L18P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|P6        |                   |IOBS     |IO_L21N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|P7        |                   |IOBM     |IO_L21P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|P8        |                   |IOBM     |IO_L19P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|P9        |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|P10       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|P11       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|P12       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|P13       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|P14       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|P15       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|P16       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|P17       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|P18       |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|P19       |                   |IOBS     |IO_L21N_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|P20       |                   |IOBM     |IO_L21P_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|P21       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|P22       |                   |IOBS     |IO_L19N_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|P23       |                   |IOBM     |IO_L19P_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|P24       |                   |IOBS     |IO_L18N_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|P25       |                   |IOBM     |IO_L18P_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|P26       |                   |         |VCCO_9              |         |           |9             |          |         |           |         |3.30     |          |         |           |                |
|R1        |                   |IOBS     |IO_L22N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|R2        |                   |IOBM     |IO_L22P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|R3        |                   |IOBS     |IO_L20N_VREF_10     |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|R4        |                   |IOBM     |IO_L20P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|R5        |                   |IOBS     |IO_L23N_VRP_10      |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|R6        |                   |IOBM     |IO_L23P_VRN_10      |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|R7        |                   |LOWCAPIOB|IO_L25N_CC_LC_10    |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|R8        |                   |LOWCAPIOB|IO_L25P_CC_LC_10    |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|R9        |                   |         |VCCO_10             |         |           |10            |          |         |           |         |any******|          |         |           |                |
|R10       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|R11       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|R12       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|R13       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|R14       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|R15       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|R16       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|R17       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|R18       |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|R19       |gpio<20>           |IOB      |IO_L25N_CC_LC_9     |BIDIR    |LVCMOS33   |9             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|R20       |gpio<21>           |IOB      |IO_L25P_CC_LC_9     |BIDIR    |LVCMOS33   |9             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|R21       |                   |IOBS     |IO_L23N_VRP_9       |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|R22       |                   |IOBM     |IO_L23P_VRN_9       |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|R23       |                   |IOBS     |IO_L22N_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|R24       |                   |IOBM     |IO_L22P_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|R25       |                   |IOBS     |IO_L20N_VREF_9      |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|R26       |                   |IOBM     |IO_L20P_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|T1        |                   |LOWCAPIOB|IO_L24N_CC_LC_10    |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|T2        |                   |         |VCCO_10             |         |           |10            |          |         |           |         |any******|          |         |           |                |
|T3        |                   |IOBS     |IO_L26N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|T4        |                   |IOBM     |IO_L26P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|T5        |                   |         |VCCO_10             |         |           |10            |          |         |           |         |any******|          |         |           |                |
|T6        |                   |IOBS     |IO_L27N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|T7        |                   |IOBM     |IO_L27P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|T8        |                   |IOBM     |IO_L31P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|T9        |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|T10       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|T11       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|T12       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|T13       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|T14       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|T15       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|T16       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|T17       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|T18       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|T19       |sram_flash_addr<21>|IOB      |IO_L31N_9           |OUTPUT   |LVDCI_33   |9             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|T20       |                   |IOBS     |IO_L30N_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|T21       |flash_a23          |IOB      |IO_L30P_9           |OUTPUT   |LVDCI_33   |9             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|T22       |                   |         |VCCO_9              |         |           |9             |          |         |           |         |3.30     |          |         |           |                |
|T23       |                   |LOWCAPIOB|IO_L24N_CC_LC_9     |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|T24       |                   |LOWCAPIOB|IO_L24P_CC_LC_9     |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|T25       |                   |         |VCCO_9              |         |           |9             |          |         |           |         |3.30     |          |         |           |                |
|T26       |gpio<19>           |IOB      |IO_L26P_9           |BIDIR    |LVCMOS33   |9             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|U1        |                   |LOWCAPIOB|IO_L24P_CC_LC_10    |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|U2        |                   |IOBS     |IO_L28N_VREF_10     |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|U3        |                   |IOBM     |IO_L28P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|U4        |                   |IOBS     |IO_L29N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|U5        |                   |IOBS     |IO_L32N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|U6        |                   |IOBM     |IO_L32P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|U7        |                   |IOBS     |IO_L31N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|U8        |                   |         |VCCO_10             |         |           |10            |          |         |           |         |any******|          |         |           |                |
|U9        |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|U10       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|U11       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|U12       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|U13       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|U14       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|U15       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|U16       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|U17       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|U18       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|U19       |                   |         |VCCO_9              |         |           |9             |          |         |           |         |3.30     |          |         |           |                |
|U20       |sram_flash_addr<22>|IOB      |IO_L31P_9           |OUTPUT   |LVDCI_33   |9             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|U21       |                   |IOBS     |IO_L29N_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|U22       |sace_usb_a<0>      |IOB      |IO_L29P_9           |OUTPUT   |LVCMOS33   |9             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|U23       |gpio<17>           |IOB      |IO_L27P_9           |BIDIR    |LVCMOS33   |9             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|U24       |gpio<14>           |IOB      |IO_L28N_VREF_9      |BIDIR    |LVCMOS33   |9             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|U25       |gpio<15>           |IOB      |IO_L28P_9           |BIDIR    |LVCMOS33   |9             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|U26       |gpio<18>           |IOB      |IO_L26N_9           |BIDIR    |LVCMOS33   |9             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|V1        |                   |IOBS     |IO_L30N_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|V2        |                   |IOBM     |IO_L30P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|V3        |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|V4        |                   |IOBM     |IO_L29P_10          |UNUSED   |           |10            |          |         |           |         |         |          |         |           |                |
|V5        |usb_hpi_int        |IOB      |IO_L2N_8            |INPUT    |LVCMOS33   |8             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|V6        |opb_error          |IOB      |IO_L2P_8            |OUTPUT   |LVCMOS33   |8             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|V7        |sram_cen           |IOB      |IO_L3N_8            |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|V8        |                   |         |VCCO_8              |         |           |8             |          |         |           |         |3.30     |          |         |           |                |
|V10       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|V11       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|V12       |                   |         |VCCO_0              |         |           |0             |          |         |           |         |any******|          |         |           |                |
|V13       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|V14       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|V15       |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|V16       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|V17       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.5      |          |         |           |                |
|V19       |                   |         |VCCO_7              |         |           |7             |          |         |           |         |2.50     |          |         |           |                |
|V20       |gpio_exp_hdr1<1>   |IOB      |IO_L5N_7            |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|V21       |gpio_exp_hdr1<22>  |IOB      |IO_L1P_7            |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|V22       |gpio_exp_hdr1<21>  |IOB      |IO_L1N_7            |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|V23       |gpio<16>           |IOB      |IO_L27N_9           |BIDIR    |LVCMOS33   |9             |2         |SLOW     |PULLDOWN   |NONE     |         |LOCATED   |         |NO         |NONE            |
|V24       |                   |         |GND                 |         |           |              |          |         |           |         |         |          |         |           |                |
|V25       |                   |IOBS     |IO_L32N_9           |UNUSED   |           |9             |          |         |           |         |         |          |         |           |                |
|V26       |sram_mode          |IOB      |IO_L32P_9           |OUTPUT   |LVDCI_33   |9             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|W1        |uart_TX            |IOB      |IO_L1N_8            |OUTPUT   |LVCMOS33   |8             |12        |SLOW     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|W2        |uart_RX            |IOB      |IO_L1P_8            |INPUT    |LVCMOS33   |8             |          |         |           |NONE     |         |LOCATED   |         |NO         |NONE            |
|W3        |sram_flash_addr<11>|IOB      |IO_L4N_VREF_8       |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|W4        |sram_adv_ld_n      |IOB      |IO_L4P_8            |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|W5        |sram_flash_addr<13>|IOB      |IO_L5N_8            |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|W6        |sram_flash_addr<12>|IOB      |IO_L5P_8            |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|W7        |flash_ce           |IOB      |IO_L3P_8            |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|W8        |                   |         |VCCO_8              |         |           |8             |          |         |           |         |3.30     |          |         |           |                |
|W9        |                   |         |VCCO_8              |         |           |8             |          |         |           |         |3.30     |          |         |           |                |
|W10       |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|W11       |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|W12       |                   |         |TCK_0               |         |           |              |          |         |           |         |         |          |         |           |                |
|W13       |                   |         |PWRDWN_B_0          |         |           |              |          |         |           |         |         |          |         |           |                |
|W14       |                   |         |M2_0                |         |           |              |          |         |           |         |         |          |         |           |                |
|W15       |                   |         |M0_0                |         |           |              |          |         |           |         |         |          |         |           |                |
|W16       |                   |         |VCCAUX              |         |           |              |          |         |           |         |2.5      |          |         |           |                |
|W17       |                   |         |VCCO_7              |         |           |7             |          |         |           |         |2.50     |          |         |           |                |
|W18       |                   |         |VCCO_7              |         |           |7             |          |         |           |         |2.50     |          |         |           |                |
|W19       |gpio_exp_hdr2<2>   |IOB      |IO_L18N_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|W20       |gpio_exp_hdr1<27>  |IOB      |IO_L5P_7            |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|W21       |gpio_exp_hdr1<26>  |IOB      |IO_L3P_7            |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|W22       |gpio_exp_hdr1<23>  |IOB      |IO_L3N_7            |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|W23       |gpio_exp_hdr2<7>   |IOB      |IO_L4P_7            |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|W24       |gpio_exp_hdr2<6>   |IOB      |IO_L4N_VREF_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|W25       |gpio_exp_hdr1<4>   |IOB      |IO_L2P_7            |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|W26       |gpio_exp_hdr1<8>   |IOB      |IO_L2N_7            |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|Y1        |sram_flash_addr<0> |IOB      |IO_L6N_8            |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|Y2        |sram_flash_addr<1> |IOB      |IO_L6P_8            |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|Y3        |sram_bw<3>         |IOB      |IO_L8N_CC_LC_8      |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|Y4        |sram_bw<2>         |IOB      |IO_L8P_CC_LC_8      |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|Y5        |sram_bw<1>         |IOB      |IO_L9N_CC_LC_8      |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|Y6        |sram_bw<0>         |IOB      |IO_L9P_CC_LC_8      |OUTPUT   |LVDCI_33   |8             |          |NONE*    |NONE**     |         |         |LOCATED   |         |NO         |DRIVER          |
|Y7        |sace_usb_a<4>      |IOB      |IO_L20N_VREF_8      |OUTPUT   |LVCMOS33   |8             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|Y8        |sace_usb_wen       |IOB      |IO_L26N_8           |OUTPUT   |LVCMOS33   |8             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|Y9        |sace_usb_a<6>      |IOB      |IO_L21N_8           |OUTPUT   |LVCMOS33   |8             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|Y10       |sace_usb_a<1>      |IOB      |IO_L27P_8           |OUTPUT   |LVCMOS33   |8             |8         |FAST     |NONE**     |         |         |LOCATED   |         |NO         |NONE            |
|Y11       |                   |         |TMS_0               |         |           |              |          |         |           |         |         |          |         |           |                |
|Y12       |                   |         |TDI_0               |         |           |              |          |         |           |         |         |          |         |           |                |
|Y13       |                   |         |TDO_0               |         |           |              |          |         |           |         |         |          |         |           |                |
|Y14       |                   |         |DOUT_BUSY_0         |         |           |              |          |         |           |         |         |          |         |           |                |
|Y15       |                   |         |M1_0                |         |           |              |          |         |           |         |         |          |         |           |                |
|Y16       |                   |         |VBATT_0             |         |           |              |          |         |           |         |         |          |         |           |                |
|Y17       |gpio_exp_hdr2<13>  |IOB      |IO_L27P_SM5_7       |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|Y18       |gpio_exp_hdr2<0>   |IOB      |IO_L21N_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|Y19       |gpio_exp_hdr2<3>   |IOB      |IO_L18P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|Y20       |gpio_exp_hdr2<5>   |IOB      |IO_L20P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|Y21       |gpio_exp_hdr2<4>   |IOB      |IO_L20N_VREF_7      |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|Y22       |gpio_exp_hdr2<9>   |IOB      |IO_L12P_7           |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|Y23       |gpio_exp_hdr2<8>   |IOB      |IO_L12N_VREF_7      |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|Y24       |gpio_exp_hdr1<6>   |IOB      |IO_L8N_CC_LC_7      |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|Y25       |gpio_exp_hdr1<10>  |IOB      |IO_L6P_7            |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
|Y26       |gpio_exp_hdr1<9>   |IOB      |IO_L6N_7            |BIDIR    |LVCMOS25   |7             |12        |SLOW     |NONE**     |NONE     |         |LOCATED   |         |NO         |NONE            |
+----------+-------------------+---------+--------------------+---------+-----------+--------------+----------+---------+-----------+---------+---------+----------+---------+-----------+----------------+

* Default value.
** This default Pullup/Pulldown value can be overridden in Bitgen. 
****** This value can be any of the allowed voltages 
       (1.2v,1.5v,1.8v,2.5v,3.3v) or VCCAUX 


